/**
  ******************************************************************************
  * @file    Project/STM32F10x_StdPeriph_Template/stm32f10x_it.c 
  * @author  MCD Application Team
  * @version V3.5.0
  * @date    08-April-2011
  * @brief   Main Interrupt Service Routines.
  *          This file provides template for all exceptions handler and 
  *          peripherals interrupt service routine.
  ******************************************************************************
  * @attention
  *
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  *
  * <h2><center>&copy; COPYRIGHT 2011 STMicroelectronics</center></h2>
  ******************************************************************************
  */

/* Includes ------------------------------------------------------------------*/
#include "stm32f10x_it.h"
#include "usart.h"
#include "string.h"
/** @addtogroup STM32F10x_StdPeriph_Template
  * @{
  */

/* Private typedef -----------------------------------------------------------*/
/* Private define ------------------------------------------------------------*/
/* Private macro -------------------------------------------------------------*/
/* Private variables ---------------------------------------------------------*/
/* Private function prototypes -----------------------------------------------*/
/* Private functions ---------------------------------------------------------*/

/******************************************************************************/
/*            Cortex-M3 Processor Exceptions Handlers                         */
/******************************************************************************/

/**
  * @brief  This function handles NMI exception.
  * @param  None
  * @retval None
  */
void NMI_Handler(void)
{
}

/**
  * @brief  This function handles Hard Fault exception.
  * @param  None
  * @retval None
  */
void HardFault_Handler(void)
{
  /* Go to infinite loop when Hard Fault exception occurs */
  while (1)
  {
  }
}

/**
  * @brief  This function handles Memory Manage exception.
  * @param  None
  * @retval None
  */
void MemManage_Handler(void)
{
  /* Go to infinite loop when Memory Manage exception occurs */
  while (1)
  {
  }
}

/**
  * @brief  This function handles Bus Fault exception.
  * @param  None
  * @retval None
  */
void BusFault_Handler(void)
{
  /* Go to infinite loop when Bus Fault exception occurs */
  while (1)
  {
  }
}

/**
  * @brief  This function handles Usage Fault exception.
  * @param  None
  * @retval None
  */
void UsageFault_Handler(void)
{
  /* Go to infinite loop when Usage Fault exception occurs */
  while (1)
  {
  }
}

/**
  * @brief  This function handles SVCall exception.
  * @param  None
  * @retval None
  */
void SVC_Handler(void)
{
}

/**
  * @brief  This function handles Debug Monitor exception.
  * @param  None
  * @retval None
  */
void DebugMon_Handler(void)
{
}

/**
  * @brief  This function handles PendSVC exception.
  * @param  None
  * @retval None
  */
void PendSV_Handler(void)
{
}

/**
  * @brief  This function handles SysTick Handler.
  * @param  None
  * @retval None
  */
void SysTick_Handler(void)
{
}
////////////////
void EXTI9_5_IRQHandler(void)
{
 
}

//////////////
void USART1_IRQHandler(void)
{
	static uint8_t i=0,rebuf[30]={0};
	if(USART_GetITStatus(USART1, USART_IT_RXNE) != RESET)//判断接收标志
	{
		rebuf[i++]=USART_ReceiveData(USART1);//读取串口数据，同时清接收标志
		if (rebuf[0]!=add)//帧头不对
			i=0;	
		else if ((i==1)&&(rebuf[1]!=0x03))//帧头不对
			i=0;
	  else if ((i==2)&&(rebuf[2]>16))//帧头不对
			i=0;
	  else if ((i==3)&&(rebuf[3]>16))//帧头不对
			i=0;
		if(i>3)//i等于4时，已经接收到数据量字节rebuf[3]
		{
			if(i<21)
			{
			if(i==(rebuf[3]+5))//判断是否接收一帧数据完毕
			{
		      
						if(!Receive_ok)//当数据处理完成后才接收新的数据
						{
							memcpy(usart_rx_data,rebuf,i);//拷贝接收到的数据
							Receive_ok=1;//接收完成标志
						}
							i=0;//缓存清0	
			
			}
			}
		}
	}
		
}

/******************************************************************************/
/*                 STM32F10x Peripherals Interrupt Handlers                   */
/*  Add here the Interrupt Handler for the used peripheral(s) (PPP), for the  */
/*  available peripheral interrupt handler's name please refer to the startup */
/*  file (startup_stm32f10x_xx.s).                                            */
/******************************************************************************/

/**
  * @brief  This function handles PPP interrupt request.
  * @param  None
  * @retval None
  */
/*void PPP_IRQHandler(void)
{
}*/

/**
  * @}
  */ 


/******************* (C) COPYRIGHT 2011 STMicroelectronics *****END OF FILE****/
